**GX-2009 Description**

72-0314RKC GX-2009, 4 gas, LEL / O2 / H2S / CO with alligator clip and 115 / 220 VAC charger

72-0314RKC-52 Confined space kit including a GX-2009 with 115 VAC charger, hand aspirator assembly with 10’ hose, probe, 34AL cyl H2S (25 ppm)/CO/O2/CH4, reg with gauge & knob, screwdriver, padded case, calibration cap, and cal tubing

**GX-2012 Description**

72-0290-22-A GX-2012, 4 sensor, LEL / O2 / H2S / CO with alkaline battery pack

72-0290-22-A-51 GX-2012 bundle, 4 sensors, LEL / O2 / H2S / CO unit with alkaline battery pack, 34AL cyl H2S/CO/O2/CH4, demand flow regulator, tubing and padded case

72-0290-27-C GX-2012 bundle, 5 sensors, % volume CH4 / LEL / O2 / H2S / CO unit with Li-Ion battery pack and 115 VAC charger, 34AL cyl H2S/CO/O2/CH4, 58L cyl 100% vol CH4, demand flow regulator, tubing and padded case

72-0290-27-C-51 GX-2012 bundle, 5 sensors, % volume CH4 / LEL / O2 / H2S / CO unit with Li-Ion battery pack and 115 VAC charger, 34AL cyl H2S/CO/O2/CH4, 58L cyl 100% vol CH4, demand flow regulator, tubing and padded case

**GX-6000 Description**

72-6AXX-C GX-6000 for LEL / O2 / H2S / CO with Li-Ion battery pack and 115 VAC charger

72-6AXX-C-51 GX-6000 for LEL / O2 / H2S / CO with Li-Ion battery pack, 115 VAC charger, 34AL cylinder CH4/O2/CO/H2S, demand flow regulator, tubing, and padded carrying case

72-6ABX-C GX-6000 for LEL / O2 / H2S / CO / VOC’s (0 - 6,000 ppm PID) with Li-Ion battery pack and 115 VAC charger

72-6ABX-C-51 GX-6000 for LEL / O2 / H2S / CO / VOC’s (0 - 6,000 ppm PID) with Li-Ion battery pack, 115 VAC charger, 34AL cylinder isobutylene/CH4/O2/CO/H2S, demand flow regulator, tubing, and padded carrying case

**EAGLE 2 Description**

724-001 EAGLE 2 for LEL & PPM / O2 / H2S / CO

724-001-50 EAGLE 2 for LEL & PPM / O2 / H2S / CO, 58AL H2S/CO/O2/CH4, dem flow reg, tubing, and padded carrying case